Bill of Material

3.1 Chassis
	Part No
	number
	Title
	Material
	Dimensions

	101
	2
	Girder
	Mild steel
	20 x 10 x 420

	102
	2
	Sittings
	Alu
	20 x 20 x 8

	103
	2
	Endplate
	copper
	140 x 55 x 1

	104
	1
	Turntable
	Brass
	( 95 x 25

	105
	8
	Hose brackets
	Brass
	5 x 1

	106
	2
	Clamp
	Brass
	20 x 180 x 3

	107
	1
	Strengthening plate
	Brass
	40 x 12 x 3

	108
	1
	Curved sheet
	Brass
	150 x 200 x 1

	109
	3
	Cross piece
	Brass
	5 x 1 x 200

	110
	4
	Spring brackets
	Mild steel
	20 x 35 x 3

	111
	2
	Sittings
	Alu
	20 x 20 x 8

	112
	2
	Side members
	Mild steel
	6 x 8 x 220

	113
	1
	Front beam
	Mild steel
	6 x 6 x 190

	114
	2
	Cross members
	Mild steel
	6 x 8 x 114

	115
	4
	Spring brackets
	Mild steel
	25 x 15 x 2,5

	116
	1
	Shaft shoe
	Brass
	6 x 1,5 x 80

	117
	1
	Turntable
	Brass
	110 x 130 x 3

	118
	2
	Hook
	Brass
	15 x 25 x 6

	119
	2
	Eye bold
	Brass
	( 6 x 20

	120
	4
	Slope iron
	Mild steel
	7 x 2 x 20

	121
	4
	Slope iron
	Mild steel
	7 x 2 x 30

	122
	1
	Bunker
	Brass
	135 x 210 x 1

	123
	1
	Sliding plate
	Brass
	50 x 105 x 1

	124
	2
	Corner profiles
	Brass
	10 x 10 x 1 x 50

	125
	2
	Corner profiles
	Brass
	5 x 5 x 1 x 50

	126
	2
	Shaft bracket
	Brass
	20 x 20 x 16

	127
	2
	Torque arm
	Mild steel
	8 x 10 x 40

	128
	2
	Crank arm
	Mild steel
	( 8 x 80

	129
	1
	Keep plate
	Mild steel
	6 x 12 x 2,5

	130
	2
	Shoe
	Brass
	7 x 10 x 25

	131
	2
	Brake pad
	Tufnol
	3 x 10 x 25

	132
	1
	Shank
	Brass
	6 x 3 x 40

	133
	1
	Step plate
	Brass
	12 x 20 x 1,6

	134
	2
	Eye bolt
	Brass
	See drawing

	135
	2
	Brake lever
	Mild steel
	210 x 8 x 2,5

	136
	2
	Handle
	Brass
	( 8 x 35

	137
	2
	Bracket
	Brass
	10 x 20 x 8

	138
	1
	Rotary part
	Mild steel
	( 6 x 95

	139
	1
	Rotary part
	Mild steel
	( 6 x 65

	140
	2
	Tension rod
	Mild steel
	( 2,5 x 220

	141
	2
	Fork head
	Brass
	6 x 6 x 10

	142
	2
	Bolt
	Brass
	( 5 x 10

	143
	2
	Rack
	Brass
	5 x 10 x 60

	144
	2
	Lamp bracket
	Brass
	35 x 20 x 3

	145
	2
	Lever guard
	Brass
	( 3 x 80


